|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **QUERY** | **SECP RESPONSE** |
| **NETWORK SWITCHES PROCUREMENT QUERIES** | | |
| 1. | Passive work requirement for Wireless Access Points? | No. Passive work is not required. |
| 2. | Manageability of Wireless Access Points? | Yes. WAPs must be manageable via controller. |
| 3. | Switches installation required or not? | No. Switches installation is not required. |
| 4. | Is rack space available for switches? | Yes. Rack space for switches is available. |
| 5. | Combo ports in new switches? | Yes. Combo/SFP ports are required. |
| 6. | Warranty requirement for switches? | 1 Year comprehensive warranty. |
| 7. | Multi-mode SFP/cable length? | Switches are in close vicinity from ODF, long length cables/SFPs are not needed. |
| 8. | Current connectivity of SECP? | End to end Gigabit. |
| 9. | SFP required for switches? | Multi-Mode SFPs are required. |
| 10. | Single power supply for switches or redundant? | Single PSU is required. Redundant power supply for switches may be quoted as optional. |
| 11. | POE Switches required? | No, POE switches are not required. |
| 12. | SFPs required with switches? | Yes, SFPs are required. |
| **SERVERS PROCUREMENT QUERIES** | | |
| 1. | Number of Virtual Machines hosted in SECP? | Approx. 200 |
| 2. | Number of physical servers at SECP? | Approx. 25 |
| 3. | Virtualization Technology at SECP? | Currently VMware, Hyper-V is a candidate for future |
| 4. | PSU requirement for servers? | Redundant PSUs are required for the servers. |
| 5. | Server installation requirement? | No, server installation is not required. |
| 6. | Branded servers are required? | Yes |
| 7. | Intel is included? | Yes, bidders are welcome to quote Intel as well. |
| 8. | IP KVM/ console redirection is required? | Yes, console redirection is required for servers, and out of band management is also required. |
| 9. | 15K RPM is required for server disks? | Yes, 15K RPM disks are required. |
| 10. | Server sockets? | Most of the servers are 2 socket, a few high end servers have 4 sockets. |
| **BACKUP SOLUTION PROCUREMENT QUERIES** | | |
| 1. | Existing backup software? | Symantec Backup Exec 2010 R3 |
| 2. | Operating system backup requirement? | Windows and Linux, VMs and physical servers. |
| 3. | Licensing model requirement for Backup Solution? | Both agent and data volume based license options may be quoted. Looking for software option only. |
| 4. | NDMP based backup license required? | Yes. LAN-free back is required. |
| 5. | Backup solution for System Center? | Currently not deployed. Backup of system center will be a requirement with the new backup solution. |
| 6. | Existing backup mechanism? | Tape library IBM TS3100 with FC connectivity. |
| **SYSTEM CENTER 2012 PROCUREMENT QUERIES** | | |
| 1. | SCCM software modules requirement? | Whole suite is required. This is a new deployment of system center. |
| 2. | Support requirement for System Center? | SA with remote support. |
| 3. | Training requirement for System Center? | Following modules trainings are required for two resources at least:   * SCCM * SCOM * SCSM * SCVMM |
| 4. | CAL requirement for System Center | Yes, 30 CALs are required. |
| 5. | System Center High Availability requirement? | Not required. |
| 6. | Installation requirement for SCCM? | Same site (single site). |
| 7. | Base Operating System requirement? | Windows Server 2012 R2. |
| 8. | Current Active Directory infrastructure? | Currently Microsoft Windows Server 2008 R2 planning to upgrade to Server 2012 R2. |
| 9. | Current software push to clients methodology? | Via Group Policy. |
| 10. | User distribution in SECP and access rights? | All internal users with roles segregation and permission levels. |
| 11. | SSL is required? | SECP will manage SSL requirements at its own. |
| 12. | WUS will be integrated with system center? | Currently WUS is running and it will be integrated with system center. |
| 13. | Any external modules licensing required, like Juniper? | No, not required at the moment. |
| **MISCELLANEOUS QUERIES** | | |
| 1. | Bid opening date? | Saturday, June 27, 2015 |
| 2. | Separate opening of technical and financial proposals? | No, single/one stage |
| 3. | Bidding currency requirement? | Pakistani Rupee (PKR) |
| 4. | Bid validity requirement? | 150 days standard validity is required however this will close by June 30th. |
| 5. | Financial criteria for bidding? | Already published on SECP website. |
| 6. | Financial format for bidding? | No particular format, any format is acceptable with 2% bid money with GST included. |
| 7. | Payment terms for SECP? | 100% after delivery. |